detachInterrupt()

[External Interrupts]

Description

Turns off the given interrupt.

Syntax

detachInterrupt(digitalPinToInterrupt(pin)) (recommended)  
detachInterrupt(interrupt) (not recommended)  
detachInterrupt(pin) (Not recommended. Additionally, this syntax only works on Arduino SAMD Boards, Uno WiFi Rev2, Due, and 101.)

Parameters

interrupt: the number of the interrupt to disable (see [attachInterrupt()](https://www.arduino.cc/reference/en/language/functions/external-interrupts/attachinterrupt) for more details).  
pin: the Arduino pin number of the interrupt to disable

Returns

Nothing