interrupts()

[Interrupts]

Description

Re-enables interrupts (after they’ve been disabled by [nointerrupts()](https://www.arduino.cc/reference/en/language/functions/interrupts/nointerrupts). Interrupts allow certain important tasks to happen in the background and are enabled by default. Some functions will not work while interrupts are disabled, and incoming communication may be ignored. Interrupts can slightly disrupt the timing of code, however, and may be disabled for particularly critical sections of code.

Syntax

interrupts()

Parameters

None

Returns

Nothing

Example Code

The code enables Interrupts.

void setup() {}

void loop() {

noInterrupts();

// critical, time-sensitive code here

interrupts();

// other code here

}